**COMPONENTS OF CISCO PACKET TRACER**  
NETWORK DEVICES  
> devices available

* 4331
* 4321
* 1941
* 2901
* 2911
* 819IOX
* 819HGW
* 8291240
* Router-PT
* Router-PT empty
* 1841
* 2621XM
* 2620XM
* 2811

>End devices

* PC
* Laptop
* Server
* Meraki-Server
* Network controller
* Printer
* IP phone0
* VoIP device
* Phone
* TV
* Tablet
* Smart phone
* Generic wireless
* Generic wired
* Sniffer

>Components

* MCU board
* SBC board
* Thing

>Connections

* Automatically choose connection type
* Console
* Copper straight – through
* Copper cross – over
* Fiber
* Phone
* Coaxial
* Serial DCE
* Serial DTE
* Octal
* IOT custom cable
* USB

>Miscellaneous

* 1841
* 2621XM
* 2811
* 2960
* Laptop
* PC

>Multi user connection

* Multi user

>Switches

* 2960
* PT Switch
* PT Empty
* 3560-24PS(multilayer switch)
* 3650-24PS(multilayer switch)
* IE-2000
* PT-bridge
* 2950-24
* 2550T

>Hubs

* PT-hub
* PT-repeater
* Coaxial splitter

>wireless devices

* Meraki
* LAP-PT
* 3702i
* WLC
* 3504
* 2504
* Home router
* AP-PT
* AP-PT-A
* AP-PT-AC
* AP-PT-N
* WRT300N
* Home gateway
* Cell tower
* CO server

>Security

* 5506
* 5505

>WAN emulation

* PT-cloud
* PT-empty
* DSL modern
* Cable modern

>Tool

* Drawing palette
* Custom devices dialog
* Script project manager
* Cluster association dialog